## Installation procedure for Raspberry Pi

* Prepare a MicroSD card with NOOBS
* Insert into Pi, and boot
* Install Raspbian
* sudo apt-get update
* sudo apt-get install tightvncserver
  + To start it, run vncserver :1 –geometry 1280x720 –depth 24
  + To connect, use TightVNC, <ip-address>:5901
* sudo apt-get install gcc-avr binutils-avr avr-libc avrdude
* sudo apt-get install apache2
* sudo apt-get install arduino
* Enable sound on headphone jack
  + amixer cset numid=3 1